1      iModelStyle (0 = airplane / 1 = helicopter)

2.0    Mass (MASS) [ kg ]
0.10   Moment of inertia around the vertical axis (fIHochachse) 
0.10   Moment of inertia around the transverse axis (fIQuerachse)
0.10   Moment of inertia around the longitudinal axis (fILaengsachse) 
2.0    Rotation resistance

30     Exponentially Elevator (expnick) [ % ]
30     Exponentially roll (exproll) [ % ]
0      Exponentially Gier (expgier) [%]
0      Exponentially Pitch (exppitch) [%]

0.65   A main rotor blade (lRot) [ m lengthens ]
0.055   Surface of the entire main rotor (aRot) [ m^2 ]
1700   Revolutions per minute of the main rotor (upmRot) [ 1/min ] 
0.10   Collective blade control of the main rotor (akol) [ wheel ] 
0.008  Cyclic blade control nodding the main rotor (azykln) [ wheel ] 
0.008  Cyclic blade control roles of the main rotor (azykln) [ wheel ] 
0.10   Height of the Rotos over the emphasis (hRot) [ m ]
0.005  Back turning inclination by horizontal incident flow (fhorzd) 

0.125   A tail rotor blade (lRoth) [ m lengthens ]
0.020  Surface of the entire tail rotor (aRoth) [ m^2 ]
7200   Revolutions per minute of the tail rotor (upmRoth) [ 1/min ] 
0.12   Collective blade control of the tail rotor (akolh) [ wheel ] 
0.009  Basic angle of incidence of the tail rotor (alpha0h) [ wheel ] 
0.75    Distance of the tail rotor axle of the emphasis (LH) [ m ] 
0.25   Greed inclination by lateral incident flow (fhorzdh)

0.03   Sensitivity of the gyroscope (hstab) [ rad/(rad/s) ] // - 0,007 = 0%, 0,05=100% 
80     Per cent of fading out the gyroscope with was appropriate the tail rotor (hstabdel) [ for % ] 

6.2    Lift rise (DCA)
1      Max. coefficient of lift (camax)
-1     Minimum coefficient of lift (camin)
0.02   Coefficient of drag with zero lift (cw0)
0.02   Resistance rise (dcw)
0.3    Coefficient of drag of the trunk (cwR)

9      Points of chassis:

0.3    PosX
0.3    PosY
-0.15  PosZ
1.0    mueh
2000   h [N/m]
10     muev
800    fmax

0.3    PosX
-0.3   PosY
-0.15  PosZ
1.0    mueh
2000   h [N/m]
10     muev
800    fmax

-0.2   PosX
-0.2   PosY
-0.15  PosZ
1.0    mueh
2000   h [N/m]
10     muev
800    fmax

-0.2   PosX
0.2    PosY
-0.15  PosZ
1.0    mueh
2000   h [N/m]
10     muev
800    fmax

-0.8   PosX
0      PosY
-0.09  PosZ
2      mueh
2500   h [N/m]
10     muev
50     fmax

0.5    PosX
0.5    PosY
0.1    PosZ
2      mueh
2500   h [N/m]
10     muev
5      fmax

0.5    PosX
-0.5   PosY
0.1    PosZ
2      mueh
2500   h [N/m]
10     muev
5      fmax

-0.5   PosX
-0.5   PosY
0.1    PosZ
2      mueh
2500   h [N/m]
10     muev
5      fmax

-0.5   PosX
0.5    PosY
0.1    PosZ
2      mueh
2500   h [N/m]
10     muev
5      fmax